Auto-tuning

* Enable Input - Asserting this input energizes the motor shaft.
* Input A - Asserting this input will make ClearPath continue to servo to its current position regardless of any changes to the frequency on Input B. Alternatively, this signal can be used as a home sensor input.
* Input B - This input is connected to a digital signal whose frequency represents the desired position.
* Output (HLFB) - See HLFB section for available modes.



